Each project's hex folder contains an executable hex file that should run when uploaded.
Use the Serial Plotter in Arduino IDE 1.8.19 to display graphs.
nRF54_Peripheral_C was used for battery-powered experiments and current measurement.